# [Edit]

1. [General]
   1. [IP/DNS]
   2. [Description]
   3. [Type]
2. [If active update process is detected on the remote node, HPSUM should]

   1. [Leave the update running and bypass the node]
   2. [Stop any currently running update process on the node and replace it with updates from this session]
3. [Prerequisites installation option]
   1. [Install iLO Channel Interface Driver if not already installed]
      [Warning: if CHIF driver is not already installed, inventory an recomemnded updates may be incomplete on Gen9 and older generation servers. Gen10 servers require CHIF driver to be installed]
4. [Baseline to Apply]
   1. [Node needs to be removed]

   2. [Remove node from the group]
   3. [Optional. Select an already added and inventoried baseline and/or additional package to apply to this node. If not added now, a baseline or additional package must be specified when Inventory is started on the node.]

   1. [Current Baseline selected]
   2. [Baseline]
   3. [Additional Package selected]
   4. [Additional Packages]
5. [Credentials]
   [Note: iLO domain credentials cannot be used to update an iLO Recovery Install Set.]
   1. [Enter Administrator Credentials]
   2. [Enter SSH key credentials]
   1. [Username]
   2. [Password]
   1. [Username] [Required]
   2. [Required]
   3. [Passphrase]
   4. [Required only if a passphrase is required for the private key file]
   [iLO CM Administrator Credentials]

   1. [Username]
   2. [Password]
   [Switch Credentials]

   [Credentials are not set for the switch]
   [Password Authentication(Applies to XGc only)]
   [Full Authentication]
   1. [Username]
      [Required] [Username not required]
   2. [Password]
      [Password not required]
   3. [Enable Password]
      [Enable Password not required]
   1. [Credentials are the same on both switches]

   [Switch B Credentials]

   [Credentials are not set for the switch B]
   [Password Authentication(Applies to XGc only)]
   [Full Authentication]
   1. [Username]
      [Required] [Username not required]
   2. [Password]
      [Password not required]
   3. [Enable Password]
      [Enable Password not required]
6. [VCenterCredentials]
   1. [Use VCenter]
   1. [IP/DNS] [Required]
   2. [Username] [Required]
   3. [Password] [Required]
7. [Access Level]
   1. [None]
   2. [Use sudo with credentials entered above]
   3. [Enter Root user credentials to update components]
   1. [Username]
   2. [Password]
8. 2. [Use Credentials Above]
   3. [Enter Administrator Credentials]
   1. [Username]
   2. [Password]
9. [Virtual Connect Options]
   [VC Activation options]
   [Activation Order]
   1. [VC Enet Modules Activation Order]
   2. [VC FC Modules Activation Order]
   [Activation Delay]
   1. [VC Enet Modules Activation Delay]
   2. [VC FC Modules Activation Delay]
10. [iLO Credentials]
    [iLO credentials are required in addition to host OS credentials when the iLO for a server is configured in Secure standard mode or one of the high security modes. Alternately 'Require Host Authentication' setting in iLO is enabled. To perform firmware update, use an iLO account that has 'Configure iLO Settings' privileges. 'Recovery Set' privileges are necessary to update the iLO recovery set.] [Note: Only applies to systems with iLO. iLO domain credentials cannot be used to update an iLO Recovery Install Set.]
    1. [Username]
    2. [Password]
    3. [App token creation option]
    4. [Create application account if not already created]
       [SUM uses virtual NIC (VNIC) to communicate with iLO that supports VNIC. For communication using VNIC, an application account in iLO is required. Creation of application account requires iLO credentials with Administer User Accounts privilege.]
11. HPE Privacy Policy