# [Find Node Range]

1. [Enter IP Address]
   [Choose type of search to use to find nodes]
2. [Enter IP Address]
   [Start IP Address]
   [End IP Address]
   [Port to Scan]
   [Invalid IP Address or Range specified]
3. [Enter LDAP Server Address]
   [LDAP Server]
   [Username]
   [Password]
   [Max Return]
   [Invalid LDAP Server or Username or Password specified]
4. [Search in Progress]
5. [Available Nodes]

   [IP Address] | [DNS Target Name]

7. [Added Nodes]

   [IP Address] | [DNS Target Name]

# [Add Nodes]

1. [General]
2. 1. [Prerequisites installation option]
   2. [Install iLO Channel Interface Driver if not already installed]
      [Warning: if CHIF driver is not already installed, inventory an recomemnded updates may be incomplete on Gen9 and older generation servers. Gen10 servers require CHIF driver to be installed]
3. [Baseline to Apply]
   [Optional. Select an already added and inventoried baseline and/or additional package to apply to this node. If not added now, a baseline or additional package must be specified when Inventory is started on the node.]

   1. [Baseline]
   2. [Additional Packages]
4. [Credentials]
   1. [Use Current Credentials (requires existing trust relationship with the target)]
   2. [Enter Administrator Credentials]
   3. [Enter SSH key credentials]
   1. [Username] [Required]
   2. [Password] [Required]
   1. [Username] [Required]
   2. [Required]
   3. [Passphrase]
   4. [Required only if a passphrase is required for the private key file]
5. [iLO Credentials]
   [iLO credentials are required in addition to host OS credentials when the iLO for a server is configured in Secure standard mode or one of the high security modes. Alternately 'Require Host Authentication' setting in iLO is enabled.To perform firmware update, use an iLO account that has 'Configure iLO Settings' privileges. 'Recovery Set' privileges are necessary to update the iLO recovery set. [Note: Only applies to systems with iLO.]
   1. [Username]
   2. [Password]