# [Add Node]

1. [Nodes]
   1. [Select operation]
   3. [IP/DNS]
   4. [Description]
   5. [Node type]
2. 1. [If active update process is detected on the remote node, SUM should]
   2. [Leave the update running and bypass the node]
   3. [Stop any currently running update process on the node and replace it with updates from this session]
3. 1. [Prerequisites installation option]
   2. [Install iLO Channel Interface Driver if not already installed]
      [if CHIF driver is not already installed, inventory and recommended updates may be incomplete on Gen9 and older generation servers. Gen10 and above servers require CHIF driver to be installed]
4. [Baseline to Apply]
   [Optional. Select an already added and inventoried baseline and/or additional package to apply to this node. If not added now, a baseline or additional package must be specified when Inventory is started on the node.]

   1. [Baseline]
   2. [Additional Packages]
5. [Group]
   [Group Description]

   1. [Assign to]
6. [Credentials]
   1. [Use Current Credentials (requires existing trust relationship with the target)]
   2. [Enter Administrator Credentials] [Note: iLO domain credentials cannot be used to update an iLO Recovery Install Set.]
   3. [Enter SSH key credentials]
   1. [Username] [Required]
   2. [Password] [Required]
   1. [Username] [Required]
   2. [Required]
   3. [Passphrase]
   4. [Required only if a passphrase is required for the private key file]
   1. [enter Vcenter Administrator Credentials]
   1. [IP/DNS] [Required]
   2. [Username] [Required]
   3. [Password] [Required]
7. [Access Level]
   1. [None]
   2. [Use sudo with credentials entered above]
   3. [Enter Root user credentials to update components]
   1. [Username] [Required]
   2. [Password] [Required]
8. [iLO Credentials]
   [iLO credentials are required in addition to host OS credentials when the iLO for a server is configured in Secure standard mode or one of the high security modes. Alternately 'Require Host Authentication' setting in iLO is enabled.To perform firmware update, use an iLO account that has 'Configure iLO Settings' privileges. 'Recovery Set' privileges are necessary to update the iLO recovery set.] [Note: Only applies to systems with iLO. iLO domain credentials cannot be used to update an iLO Recovery Install Set.]

   1. [Username]
   2. [Password]
   3. [App token creation option]
   4. [Create application account if not already created]
      [SUM uses virtual NIC (VNIC) to communicate with iLO that supports VNIC. For communication using VNIC, an application account in iLO is required. Creation of application account requires iLO credentials with Administer User Accounts privilege.]
9. 2. [Use Credentials Above]
   3. [Enter Administrator Credentials]
      1. [Username] [Required]
      2. [Password] [Required]
10. [Credentials]
    [iLO CM Administrator Credentials]

    1. [Username] [Required]
    2. [Password] [Required]
    [Enter switch credentials (Required only if switch firmware is to be updated)]
    [Switch Credentials]

    [Credentials are not set for the switch]
    [Password Authentication(Applies to XGc only)]
    [Full Authentication]
    1. [Username]
       [Required] [Username not required]
    2. [Password]
       [Password not required]
    3. [Enable Password]
       [Enable Password not required]
    4. [Credentials are the same on both switches]

    [Switch B Credentials]

    [Credentials are not set for the switch B]
    [Password Authentication(Applies to XGc only)]
    [Full Authentication]
    1. [Username]
       [Required] [Username not required]
    2. [Password]
       [Password not required]
    3. [Enable Password]
       [Enable Password not required]
11. HPE Privacy Policy

[Search is in progress. Please wait...]

[Nodes will be populated after search.]